### Gmod-Teach-Gma

Instala en lote automaticamente mods en formato.gma y .bin

### Native .hcd firmware binaries for legacy Broadcom chips (0a5c:219c).

Fixes the continuous USB reset loop error (failed to resubmit (2)) on modern Linux kernels
(Debian 13+, Ubuntu, Arch). Ready to drop into /lib/firmware/brcm/.

bcm2070 linux driver, 0a5c:219c firmware, failed to resubmit 2 broadcom, debian 13 bluetooth fix, BCM2070A0.hcd download